<div align=center>
<img src="https://github.com/BestModules-Libraries/img/blob/main/BMS33M332_V1.0.png" width="320" height="240"> 
</div> 

BMS33M332 
===========================================================

The Best Modules BMS33M332 is a proximity sensing and ambient light detection module, which uses the I2C communication method. This document provides the description of the BMS33M332 Arduino Lib functions and how to install the Arduino Lib. The example demonstrates the function of reading A/D values for proximity sensing and ambient light.

This library can be installed via the Arduino Library manager. Search for **BMS33M332**. 

Repository Contents
-------------------

* **/examples** - Example sketches for the library (.ino). Run these from the Arduino IDE. 
* **/src** - Source files for the library (.cpp, .h).
* **keywords.txt** - Keywords from this library that will be highlighted in the Arduino IDE. 
* **library.properties** - General library properties for the Arduino package manager. 

Documentation 
-------------------

* **[BMS33M332 Arduino Library V1.0.1 Description v100]( https://www.bestmodulescorp.com/bms33m332.html#tab-product2 )** - Arduino Library Description.

Version History  
-------------------

* **V1.0.1** - Initial public release.

License Information
-------------------

This product is _**open source**_! 

Please review the LICENSE.md file for license information. 

If you have any questions or concerns on licensing, please contact technical support on our BESTMODULES Email:service@bestmodulescorp.com

Distributed as-is; no warranty is given.

BESTMODULES
