/*********************************************************************************************************//**
 * @file    BM32S2031_1_HT32/BM32S2031_1_porting_guide.txt
 * @version V1.0.1
 * @date    2024-08-22
 * @brief   Description of modules porting guide.
 *************************************************************************************************************
 * @attention
 *
 * Firmware Disclaimer Information
 *
 * 1. The customer hereby acknowledges and agrees that the program technical documentation, including the
 *    code, which is supplied by Holtek Semiconductor Inc., (hereinafter referred to as "HOLTEK") is the
 *    proprietary and confidential intellectual property of HOLTEK, and is protected by copyright law and
 *    other intellectual property laws.
 *
 * 2. The customer hereby acknowledges and agrees that the program technical documentation, including the
 *    code, is confidential information belonging to HOLTEK, and must not be disclosed to any third parties
 *    other than HOLTEK and the customer.
 *
 * 3. The program technical documentation, including the code, is provided "as is" and for customer reference
 *    only. After delivery by HOLTEK, the customer shall use the program technical documentation, including
 *    the code, at their own risk. HOLTEK disclaims any expressed, implied or statutory warranties, including
 *    the warranties of merchantability, satisfactory quality and fitness for a particular purpose.
 *
 * <h2><center>Copyright (C) Holtek Semiconductor Inc. All rights reserved</center></h2>
 ************************************************************************************************************/

 ===========================Steps for porting module to HT32 Starter Kit.===========================
 Step 1. Modify example_xxxxx\_ProjectConfig.ini.
         - Add DEVICE_NAME
         Example [take HT32F52352 as an example]:
           REM DEVICE_NAME
           REM ============================================================================
           52352

 Step 2. Modify example_xxxxx\ht32_board_config.h.
         - Add module communication interface pin setting
         Example [take HT32F52352 as an example]:
            #if defined(USE_HT32F52352_SK)
            /*----------------------------------------------------------------------------------------------------------*/
            /* UART Module Setting                                                                                      */
            /*----------------------------------------------------------------------------------------------------------*/
              #define HTCFG_UARTM_CH0                         USART1
              #define HTCFG_UARTM0_TX_GPIO_PORT               A
              #define HTCFG_UARTM0_TX_GPIO_PIN                4
              #define HTCFG_UARTM0_RX_GPIO_PORT               A
              #define HTCFG_UARTM0_RX_GPIO_PIN                5
              #define HTCFG_UARTM0_TX_BUFFER_SIZE             128
              #define HTCFG_UARTM0_RX_BUFFER_SIZE             128

            /*----------------------------------------------------------------------------------------------------------*/
            /* SPI Module Setting                                                                                       */
            /*----------------------------------------------------------------------------------------------------------*/
              #define HTCFG_CH0_SCK_GPIO_PORT                 B
              #define HTCFG_CH0_SCK_GPIO_PIN                  3
              #define HTCFG_CH0_SEL_GPIO_PORT                 B
              #define HTCFG_CH0_SEL_GPIO_PIN                  2
              #define HTCFG_CH0_MOSI_GPIO_PORT                B
              #define HTCFG_CH0_MOSI_GPIO_PIN                 4
              #define HTCFG_CH0_MISO_GPIO_PORT                B
              #define HTCFG_CH0_MISO_GPIO_PIN                 5
              #define HTCFG_SPI_CH0                           SPI0

            /*----------------------------------------------------------------------------------------------------------*/
            /* I2C Master Setting                                                                                       */
            /*----------------------------------------------------------------------------------------------------------*/
              #define HTCFG_I2CM_CH0                          I2C1
              #define HTCFG_M0_SCL_GPIO_PORT                  A
              #define HTCFG_M0_SCL_GPIO_PIN                   0
              #define HTCFG_M0_SDA_GPIO_PORT                  A
              #define HTCFG_M0_SDA_GPIO_PIN                   1
            #endif

 ===========================Steps for porting module to Another Vendor's MCU.=======================
 Step 1. Unzip File:
         - Start by unzipping "BM32S2031_1_HT32_Vm.n.r.zip".

 Step 2. Port Source Code:
         - Migrate the src directory to your target project.
         Example: D:\<Another Vendor's MCU Target Project>\src

 Step 3. Include in Compilation:
         - Open the Keil project and make modifications as below.
         (Ensure "BM32S2031_1.c" and header files are included in your project's build list.)
         1. Add the module "Include Paths" to the project.
            Example: D:\<Another Vendor's MCU Target Project>\src
         2. Add the module "C language files" to the project.
            Example: BM32S2031_1.c

 Step 4. Modify Includes and APIs:
         - Use global search to identify and modify include files and APIs for porting.
         /*
           !!! PORTING !!!
           Description...
         */
         Note : Porting this module need to implement required APIs as below:
         -       API        :           Description         -
         ====================================================
         - BM32S2031_1_selSerial()   : Module UART communication interface pin change.
         - BM32S2031_1_Init()        : Module initialization.
         - _BM32S2031_1_writeBytes() : write data.
         - _BM32S2031_1_readBytes()  : read data.
         - _BM32S2031_1_delay()      : delay ms.
