<div align=center>
<img src="https://github.com/BestModules-Libraries/img/blob/main/BMD26M088_V1.0.png" width="240" height="240"> 
</div> 

BMD26M088
===========================================================

The Best Modules BMD26M088 is a 8×8 RGB LED module, which uses the I2C communication method. This document provides the description of the BMD26M088 Arduino Lib functions and how to install the Arduino Lib. The example demonstrates the function of the light panel display.

This library can be installed via the Arduino Library manager. Search for **BMD26M088**. 

Repository Contents
-------------------

* **/examples** - Example sketches for the library (.ino). Run these from the Arduino IDE. 
* **/src** - Source files for the library (.cpp, .h).
* **keywords.txt** - Keywords from this library that will be highlighted in the Arduino IDE. 
* **library.properties** - General library properties for the Arduino package manager. 

Documentation 
-------------------

* **[BMD26M088 Arduino Library V1.0.1 Description v100]( https://www.bestmodulescorp.com/bmd26m088.html#tab-product2 )** - Arduino Library Description.

Version History  
-------------------

* **V1.0.1**  
&emsp;&emsp;- Initial public release.
* **V1.0.2**  
&emsp;&emsp;- Add functions:readCmd()、 setOverTemperatureProtect()、getOverTemperatureFlag()、setGradient();  
&emsp;&emsp;- Add examples:gradient、colorful;  
&emsp;&emsp;- Optimize function:being()-avoid power-on flickering issues;  
&emsp;&emsp;- Optimize examples:change the module address to 0X67 for all examples;  
* **V1.0.3**  
&emsp;&emsp;- Changed the I2C address of the 'colorful'and 'Gradient' examples: I2C address changed from 0x65 to 0x67；

License Information
-------------------

This product is _**open source**_! 

Please review the LICENSE.md file for license information. 

If you have any questions or concerns on licensing, please contact technical support on our BESTMODULES Email:service@bestmodulescorp.com

Distributed as-is; no warranty is given.

BESTMODULES
