<div align=center>
<img src="https://github.com/BestModules-Libraries/img/blob/main/BME34M101_V1.0.png" width="480" height="240"> 
</div> 


BME34M101
===========================================================

The Best Modules BME34M101 is a soil moisture detection module, which uses the UART communication method. This document provides the description of the BME34M101 Arduino Lib functions and how to install the Arduino Lib. The example demonstrates the function of obtaining the module soil moisture detection value and temperature value.

This library can be installed via the Arduino Library manager. Search for **BME34M101**. 

Repository Contents
-------------------

* **/examples** - Example sketches for the library (.ino). Run these from the Arduino IDE. 
* **/src** - Source files for the library (.cpp, .h).
* **keywords.txt** - Keywords from this library that will be highlighted in the Arduino IDE. 
* **library.properties** - General library properties for the Arduino package manager. 

Documentation 
-------------------

* **[BME34M101 Arduino Library V1.0.1 Description v100]( https://www.bestmodulescorp.com/bme34m101.html#tab-product2 )** - Arduino Library Description.

Version History  
-------------------

* **V1.0.1** - Initial public release.

License Information
-------------------

This product is _**open source**_! 

Please review the LICENSE.md file for license information. 

If you have any questions or concerns on licensing, please contact technical support on our BESTMODULES Email:service@bestmodulescorp.com

Distributed as-is; no warranty is given.

BESTMODULES
