<div align=center>
<img src="https://github.com/BestModules-Libraries/img/blob/main/BMP73T104_V1.0.png" width="320" height="240"> 
</div> 

BMP73T104 
===========================================================

The BMP73T104 is a shield board for four-channel motor driver from Best Modules, and uses the I2C communication mode. This document provides the description of the BMP73T104 Arduino Lib functions and how to install the Arduino Lib. The example demonstrates the functions of driving DC motor and stepper motor.


This library can be installed via the Arduino Library manager. Search for **BMP73T104**. 

Repository Contents
-------------------

* **/examples** - Example sketches for the library (.ino). Run these from the Arduino IDE. 
* **/src** - Source files for the library (.cpp, .h).
* **keywords.txt** - Keywords from this library that will be highlighted in the Arduino IDE. 
* **library.properties** - General library properties for the Arduino package manager. 

Documentation 
-------------------

* **[BMP73T104 Arduino Library V1.0.1 Description v100]( https://www.bestmodulescorp.com/bmp73t104.html#tab-product2 )** - Arduino Library Description.

Version History  
-------------------

* **V1.0.1** 
&emsp;&emsp;- Initial public release.
* **V1.0.2** 
&emsp;&emsp;- Add example:twoSteppersRun.  

License Information
-------------------

This product is _**open source**_! 

Please review the LICENSE.md file for license information. 

If you have any questions or concerns on licensing, please contact technical support on our BESTMODULES Email:service@bestmodulescorp.com

Distributed as-is; no warranty is given.

BESTMODULES
