<div align=center>
<img src="https://github.com/BestModules-Libraries/img/blob/main/BMP75M131_V1.0.png" width="300" height="240"> 
</div> 

BMP75M131
===========================================================

The BMP75M131 is a relay module from Best Modules, which uses the I2C communication method.This document provides the description of the BMP75M131 Arduino Lib functions and how toinstall the Arduino Lib. The example demonstrates the relay control and other functions.

This library can be installed via the Arduino Library manager. Search for **BMP75M131**. 

Repository Contents
-------------------

* **/examples** - Example sketches for the library (.ino). Run these from the Arduino IDE. 
* **/src** - Source files for the library (.cpp, .h).
* **keywords.txt** - Keywords from this library that will be highlighted in the Arduino IDE. 
* **library.properties** - General library properties for the Arduino package manager. 

Documentation 
-------------------

* **[BMP75M131 Arduino Library V1.0.1 Description v100](https://www.bestmodulescorp.com/bmp75m131.html#tab-product2)** - Arduino Library Description.

Version History  
-------------------

* **V1.0.1** - Initial public release.

License Information
-------------------

This product is _**open source**_! 

Please review the LICENSE.md file for license information. 

If you have any questions or concerns on licensing, please contact technical support on our BESTMODULES Email:service@bestmodulescorp.com

Distributed as-is; no warranty is given.

BESTMODULES
