<div align=center>
<img src="https://github.com/BestModules-Libraries/img/blob/main/BMS56M605_V1.0.png" width="320" height="240"> 
</div> 

BMS56M605 
===========================================================

The BMS56M605 is a gyroscope and accelerometer module from Best Modules, which uses the I2C communication method. This document provides the description of the BMS56M605 Arduino Lib functions and how to install the Arduino Lib. The example demonstrates the functions of reading the 6-axis data and motion detection.

This library can be installed via the Arduino Library manager. Search for **BMS56M605**. 

Repository Contents
-------------------

* **/examples** - Example sketches for the library (.ino). Run these from the Arduino IDE. 
* **/src** - Source files for the library (.cpp, .h).
* **keywords.txt** - Keywords from this library that will be highlighted in the Arduino IDE. 
* **library.properties** - General library properties for the Arduino package manager. 

Documentation 
-------------------

* **[BMS56M605 Arduino Library V1.0.1 Description v100]( https://www.bestmodulescorp.com/bms56m605.html#tab-product2 )** - Arduino Library Description.

Version History  
-------------------

* **V1.0.1** - Initial public release.

License Information
-------------------

This product is _**open source**_! 

Please review the LICENSE.md file for license information. 

If you have any questions or concerns on licensing, please contact technical support on our BESTMODULES Email:service@bestmodulescorp.com

Distributed as-is; no warranty is given.

BESTMODULES
