<div align=center>
<img src="https://github.com/BestModules-Libraries/img/blob/main/BMC11T001_V1.0.png" width="320" height="240"> 
</div> 

BMC11T001
===========================================================

The Best Modules BMC11T001 is a shield board for the NFC card reader function, which uses the UART communication method. This document describes the Arduino Lib functions of the BMC11T001 and how to install the Arduino Lib. The provided examples demonstrate how to implement the UID read operation, data read/write operations and other functions. 

This library can be installed via the Arduino Library manager. Search for **BMC11T001**. 

Repository Contents
-------------------

* **/examples** - Example sketches for the library (.ino). Run these from the Arduino IDE. 
* **/src** - Source files for the library (.cpp, .h).
* **keywords.txt** - Keywords from this library that will be highlighted in the Arduino IDE. 
* **library.properties** - General library properties for the Arduino package manager. 

Documentation 
-------------------

* **[BMC11T001 Arduino Library V1.0.1 Description v100]( https://www.bestmodulescorp.com/bmc11t001.html#tab-product2 )** - Arduino Library Description.

Version History  
-------------------

* **V1.0.1** - Initial public release.

License Information
-------------------

This product is _**open source**_! 

Please review the LICENSE.md file for license information. 

If you have any questions or concerns on licensing, please contact technical support on our BESTMODULES Email:service@bestmodulescorp.com

Distributed as-is; no warranty is given.

BESTMODULES
