<div align=center>
<img src="https://github.com/BestModules-Libraries/img/blob/main/BMD11M134_V1.0.png" width="320" height="240"> 
</div> 

BMD11M134
===========================================================

The Best Modules BMD11M134 is a 4-digit digital tube module, which uses the I2C communication method. This document provides the description of the BMD11M134 Arduino Lib function and how to install the Arduino Lib. The example demonstrates the function of displaying characters by using digital tubes.

This library can be installed via the Arduino Library manager. Search for **BMD11M134**. 

Repository Contents
-------------------

* **/examples** - Example sketches for the library (.ino). Run these from the Arduino IDE. 
* **/src** - Source files for the library (.cpp, .h).
* **keywords.txt** - Keywords from this library that will be highlighted in the Arduino IDE. 
* **library.properties** - General library properties for the Arduino package manager. 

Documentation 
-------------------

* **[BMD11M134 Arduino Library Description](https://www.bestmodulescorp.com/bmd11m134.html#tab-product2)** - Arduino Library Description.

Version History  
-------------------

* **V1.0.1**  
&emsp;&emsp;- Initial public release.
* **V1.0.2**  
&emsp;&emsp;- Improve function functions: begin, shiftRight, shiftLeft;  
&emsp;&emsp;- Improve the example content and update the schematic image: shift;  
&emsp;&emsp;- Perfect some function header comments.  

License Information
-------------------

This product is _**open source**_! 

Please review the LICENSE.md file for license information. 

If you have any questions or concerns on licensing, please contact technical support on our BEST MODULES CORP. Email:service@bestmodulescorp.com

Distributed as-is; no warranty is given.

BEST MODULES CORP.
