<div align=center>
<img src="https://github.com/BestModules-Libraries/img/blob/main/BM2302-9x-1_BMC23M0x1_V1.0.png" width="480" height="240"> 
</div> 

BM2302-9x-1 
===========================================================

The BM2302-9x-1 is a Sub-1G OOK receiver transparent transmission module from the Best Modules, which uses the I2C/UART communication method. This document describes the Arduino Lib function of the BM2302-9x-1 and how to install the Arduino Lib. The examples demonstrate how to use the BMC23M0x1 module to pair with the Sub-1G OOK transmitter transparent transmission module BMC21M0x1, data exchange and other functions.

#### Applicable types:
<div align=center>

|Part No.   |Description                                        |
|:---------:|:-------------------------------------------------:|
|BM2302-9x-1|Sub-1G OOK receiver transparent transmission module|
|BMC23M0x1  |On-board BM2302-9x-1 module                        |

</div> 

This library can be installed via the Arduino Library manager. Search for **BM2302-9x-1**. 

Repository Contents
-------------------

* **/examples** - Example sketches for the library (.ino). Run these from the Arduino IDE. 
* **/src** - Source files for the library (.cpp, .h).
* **keywords.txt** - Keywords from this library that will be highlighted in the Arduino IDE. 
* **library.properties** - General library properties for the Arduino package manager. 

Documentation 
-------------------

* **[BM2302-9x-1 Arduino Library V1.0.1 Description v100]( https://www.bestmodulescorp.com/bm2302-9x-1.html#tab-product2 )** - Arduino Library Description.

Version History  
-------------------

* **V1.0.1** - Initial public release.

License Information
-------------------

This product is _**open source**_! 

Please review the LICENSE.md file for license information. 

If you have any questions or concerns on licensing, please contact technical support on our BESTMODULES Email:service@bestmodulescorp.com

Distributed as-is; no warranty is given.

BESTMODULES
